# NetBIOS-Computernamen und ihr Aufbau

Gültig für: Alle Windows Versionen

NetBIOS-Namen sind immer 16-Zeichen lang. Unter Windows dürfen Sie aber nur die ersten 15-Zeichen für einen Computernamen verwenden. Das 16. Zeichen benutzt Windows, um den Typ festzulegen.

Hier eine Auflistung einiger wichtiger Typen:

NetBIOS Name (15 Zeichen) | 16 Zeichen | Typ | Bedeutung
Computername | 00 | U | Workstation Service
Domainname | 00 | G | Domain Name
IS~Computername | 00 | U | IIS
Computername | 01 | U | Messenger Service
\\--__MSBROWSE__-- | 01 | G | Master Browser
Computername | 03 | U | Messenger Service
Username | 03 | U | Messenger Service
Computername | 06 | U | RAS Server Service
Domainname | 1B | U | Domain Master Browser
Domainname | 1C | G | Domain Controllers
INet-Service | 1C | G | IIS
Domainname | 1D | U | Master Browser
Domainname | 1E | G | Browser Service Elections
Computername | 1F | U | NetDDE Service
Computername | 20 | U | File Server Service
Forte_$ND800ZA | 20 | U | DCA Ireinmalan Gateway Server Service
Computername | 21 | U | RAS Client Service
Computername | 22 | U | MS Exchange (Mail Connector)
Computername | 23 | U | MS Exchange Store
Computername | 24 | U | MS Exchange Directory
Computername | 2B | U | Lotus Notes Server Service
IRSMULTICAST | 2F | G | Lotus Notes
Computername | 30 | U | Modem Sharing Server Service
Computername | 31 | U | Modem Sharing Client Service
IRSMULTICAST | 33 | G | Lotus Notes
Computername | 43 | U | SMS Client Remote Control
Computername | 44 | U | SMS Administrator Remote Control
Computername | 45 | U | SMS Client Remote Chat
Computername | 46 | U | SMS Client Remote Transfer
Computername | 4C | U | DEC Pathworks TCPIP Service
Computername | 42 | U | McAfee Antivirus
Computername | 52 | U | DEC Pathworks TCPIP Service
Computername | 87 | U | MS Exchange MTA
Computername | 6A | U | MS Exchange IMC
Computername | BE | U | Network Monitor Agent
Computername | BF | U | Network Monitor Application

Computername, Domainname und Username sind durch die entsprechenden Namen zu ersetzen.

Folgende unterschiedliche Typen gibt es:

Typ | Beschreibung
U | Dieser Typ besitzt nur eine IP-Adresse
G | Dieser Typ besitzt mehr als eine IP-Adresse

WinFAQ: Startseite | WinFAQ: HTMLMenü | WinFAQ: Java Version

Der Tipp enthält einen Fehler oder Sie haben noch eine Ergänzung dafür? Schreiben Sie uns über die Feedback-Seite an: Feedback-Formular

URL: http://www.winfaq.de/faq_html/Content/tip1000/tip1064.htm

WinFAQ ® Version 9.01 Copyright © 1996/2016 by Frank Ullrich